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APPLICABLE  TO
Portable X-ray Machine
Shot Lumbar Spine Master
Model: PO8R
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Product features
Intelligent temperature management
10.4 inch Super large screen
3 exposure modes, easy to switching
High voltage tank build inside as monoblock
Excellent exposure time
8kW High power portable X-ray machine  

Ultra-portable, intuitive operation, exceptional imaging.
Clinical pictures
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Fast and convenient packaging,Simple transportation.
Package
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System Requirements
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Mechanics parameters
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